{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["A8_Inter_B"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"A8_Inter_B","index":0,"n_rows":64,"n_cols":6,"rows_kept":64,"cut":false,"hidden":false,"merged":[]}
[null,null,null,"A8_Inter_B 焊接BOM"]
[null,"编辑：","黄新凯","日期：2016-4-12","版本：","V1.1"]
["序号","名称","型号","规格","数量","单位"]
[1,"贴片电容","100nF/50V","0805C,精度：+-10%",80,"pcs"]
[2,"贴片电容","1000pF/2KV","1206 精度：+-10%",5,"pcs"]
[3,"贴片电容","15pF/50V","0805C,精度：+-10%",16,"pcs"]
[4,"贴片钽电容","100UF/10V","1210C,精度：+-10%",8,"pcs"]
[5,"贴片钽电容","10uF/10V","1206C,精度：+-10%",7,"pcs"]
[6,"贴片电解电容","470UF/35V","10X10.5",4,"pcs"]
[7,"贴片电阻","22R","0805R,精度：5%,1/8W",2,"pcs"]
[8,"贴片电阻","15K","0805R,精度：5%,1/8W",2,"pcs"]
[9,"贴片电阻","200R","0805R,精度：5%,1/8W",59,"pcs"]
[10,"贴片电阻","470R","0805R,精度：5%,1/8W",13,"pcs"]
[11,"贴片电阻","1K","0805R,精度：5%,1/8W",38,"pcs"]
[12,"贴片电阻","22K","0805R,精度：5%,1/8W",4,"pcs"]
[13,"贴片电阻","2K","0805R,精度：5%,1/8W",18,"pcs"]
[14,"贴片电阻","4.7K","0805R,精度：5%,1/8W",3,"pcs"]
[15,"贴片电阻","150R","0805R,精度：5%,1/8W",8,"pcs"]
[16,"贴片电阻","10k ","0805R,精度：1%,1/8W",5,"pcs"]
[17,"贴片电阻","0R","0805R,精度：5%,1/8W",1,"pcs"]
[18,"贴片电阻","75R","0805R,精度：5%,1/8W",1,"pcs"]
[19,"贴片电阻","5.6K","0805R,精度：5%,1/8W",4,"pcs"]
[20,"贴片电阻","100K","0805R,精度：5%,1/8W",2,"pcs"]
[21,"插件可调电阻","10K精密可调电阻","RW1，3P，间距2.54",1,"pcs"]
[22,"贴片三极管","S8550","SOT23 ",3,"pcs"]
[23,"贴片二极管","1N4148","1206D",4,"pcs"]
[24,"贴片二极管","1N4007","1206D",3,"pcs"]
[25,"贴片TVS管","SMBJ18.0CA","DO-214AA",16,"pcs"]
[26,"贴片TVS管","BV05C","SOD323",8,"pcs"]
[27,"贴片TVS管","SMBJ6.5CA","DO-214AA",5,"pcs"]
[28,"贴片电感","10UH","1206",3,"pcs"]
[29,"贴片电感"," 600Ω/100MHz","0805",21,"pcs"]
[30,"贴片功率电感","30UH","L10*10",2,"pcs"]
[31,"贴片保险丝","SMD1812P200TF",1812,2,"pcs"]
[32,"贴片保险丝","SMD1812P110TF","1812",6,"pcs"]
[33,"贴片发光二极管","LED","0805L",37,"pcs"]
[34,"贴片反相器IC","74LVC04","SO-14",2,"pcs"]
[35,"贴片与门IC","SN74LVC08AD","SO-14",1,"pcs"]
[36,"贴片485 IC","MAX3485E","SOP8",2,"pcs"]
[37,"插件485模块","RSM3485C-3.3V","RSM485C",2,"pcs"]
[38,"贴片232 IC","SP3223EEY","TSSOP-20",4,"pcs"]
[39,"贴片四光耦 IC","TLP521-4","TLP521-4",2,"pcs"]
[40,"贴片光耦 IC","HCPL-0600-500E","SOP8",5,"pcs"]
[41,"贴片运放IC","OP491","SO-14",2,"pcs"]
[42,"贴片稳压IC","TL431ACLP","TO-92A",1,"pcs"]
[43,"贴片AD采样 IC","TLC2543I","SOL-20",1,"pcs"]
[44,"贴片3.3V IC","ASM1117M3-3.3","SOT223",1,"pcs"]
[45,"贴片5.0V IC","ASM1117M3-5.0","SOT223",1,"pcs"]
[46,"插件电源模块","WRB1205CS-3W","WRB_CS_3W",1,"pcs"]
[47,"插件光耦","TL113","DIP6",3,"pcs"]
[48,"插件继电器","G5LA-14 12V  DC","JZC-22F",3,"pcs"]
[49,"插座RJ45*8","2*4,8口双层","RJ45-8C",3,"pcs"]
[50,"插座8PIN","8PIN端子座","8SIP5.08",1,"pcs"]
[51,"牛角连接器","HEADER 10X2","公头，2.54间距，直脚",1,"pcs"]
[52,"牛角连接器","HEADER 13X2","公头，2.54间距，直脚",1,"pcs"]
[53,"牛角连接器","HEADER 7X2","公头，2.54间距，直脚",1,"pcs"]
[54,"牛角连接器","HEADER 10X2","母头，2.54间距，带扣",null,"pcs"]
[55,"牛角连接器","HEADER 13X2","母头，2.54间距，带扣",null,"pcs"]
[56,"牛角连接器","HEADER 7X2","母头，2.54间距，带扣",null,"pcs"]
[57,"RJ45+USB插座","RJ45+USB","RJ45-HRX-1",1,"pcs"]
[58,"排针","3PIN-1","SIP3",2,"pcs"]
[59,"端子","XH2.54-2P","2.54间距，直脚",1,"pcs"]
[60,"端子","VH3.96-2p","直脚，带线长20cm ",null,"pcs"]
[61,"PCB板","A8_Inter_B ，大小：10.5*28cm\n","按PCB图下单，上传文件,材质：FR4，板厚：1.6cm，铜厚：1OZ",1,"pcs"]