{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["A8_Inter_B"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"A8_Inter_B","index":0,"n_rows":64,"n_cols":8,"rows_kept":64,"cut":false,"hidden":false,"merged":[]}
[null,null,null,"A8_Inter_B 焊接BOM"]
[null,"编辑：","黄新凯","日期：2016-4-12","版本： V1.1"]
["序号","名称","型号","规格","安装位置","数量","单位"," 备注"]
[1,"贴片电容","100nF/50V","0805C,精度：+-10%","C45 ,C48 ,C53, C54 ,C59 ,C60 ,C68 ,C69,C117 ,C118 ,C1 ,C2 ,C3 ,C4 ,C7 ,C8 ,C9, C10 ,C11 ,C12 ,C13 ,C14 ,C15 ,C16 ,C17 ,C18 ,C19  ,C20, C21 ,C22 ,C23 ,C44 ,C46 , C47 ,C49 ,C50 ,C51,C52 ,C55 ,C56 ,C57,C58 ,C61 ,C62 ,C63 ,C64 ,C65 ,C66 ,C67 , C70 ,C71 ,C72 ,C73  ,C74 ,C75 ,C76 ,C77, C78 ,C80 ,C82 ,C84 ,C85 ,C93 ,C94 ,C95 ,C96 ,C97 ,C98 ,C99 , C100 ,C104,  C119 ,C120 ,  C123, C124 , C126 ,C127 ,C128, C132 ,C133",80,"pcs"]
[2,"贴片电容","1000pF/2KV","1206 精度：+-10%","C5, C6, C129, C130, C131",5,"pcs"]
[3,"贴片电容","15pF/50V","0805C,精度：+-10%","C28, C29, C30, C31, C32, C33, C34, C35, C36, C37, C38, C39, C40, C41, C42, C43",16,"pcs"]
[4,"贴片钽电容","100UF/10V","1210C,精度：+-10%","C101, E3, E4, E5, E6, E7, E8, E9",8,"pcs"]
[5,"贴片钽电容","10uF/10V","1206C,精度：+-10%","C24, C25, C26, C27, CT2,C122, C125",7,"pcs"]
[6,"贴片电解电容","470UF/35V","10X10.5","E1,E2, E10, E11",4,"pcs"]
[7,"贴片电阻","22R","0805R,精度：5%,1/8W","R1, R2",2,"pcs"]
[8,"贴片电阻","15K","0805R,精度：5%,1/8W","R3, R4",2,"pcs"]
[9,"贴片电阻","200R","0805R,精度：5%,1/8W","R5 ,R6, R7, R8 ,R9 ,R10 , R11 ,R12 , R13 ,R14 , R15 ,R16 , R17 ,R18  ,R19,R20 ,R45 ,R46 ,R60 ,R61 , R62, R63 , R64, R65 , R66 ,R67 , R68, R69  ,R70 ,R71, R72 ,R73 , R74 ,R75,  R92 ,R108  ,R118,R119  ,R120 ,R121,  R122 ,R123, R124, R125, R126 ,R127  ,R128 ,R129 , R139 ,R140,  R141 ,R142 , R149 ,R150 , R151 ,R152, R159, R160, R161",59,"pcs"]
[10,"贴片电阻","470R","0805R,精度：5%,1/8W","R21, R22, R23, R24, R25, R26, R27, R28, R96, R97, R98, R115, R116",13,"pcs"]
[11,"贴片电阻","1K","0805R,精度：5%,1/8W","R29, R30, R31, R32, R33, R34, R35, R36, R37, R38, R39, R40, R41, R42, R43, R48, R49, R50, R51, R52, R53, R54, R55, R56, R57, R58, R59, R99, R109, R130, R132, R134, R137, R138, R147, R148, R157, R158",38,"pcs"]
[12,"贴片电阻","22K","0805R,精度：5%,1/8W","R44, R47, R146, R156",4,"pcs"]
[13,"贴片电阻","2K","0805R,精度：5%,1/8W","R76, R77, R78, R79, R80, R81, R82, R83, R84, R85, R86, R87, R88, R89, R90, R91, R110, R111",18,"pcs"]
[14,"贴片电阻","4.7K","0805R,精度：5%,1/8W","R93, R94, R95",3,"pcs"]
[15,"贴片电阻","150R","0805R,精度：5%,1/8W","R100, R101, R102, R103, R104, R105, R106, R107",8,"pcs"]
[16,"贴片电阻","10k ","0805R,精度：1%,1/8W","R112, R113,R131, R133, R135",5,"pcs"]
[17,"贴片电阻","0R","0805R,精度：5%,1/8W","R117",1,"pcs"]
[18,"贴片电阻","75R","0805R,精度：5%,1/8W","R136",1,"pcs"]
[19,"贴片电阻","5.6K","0805R,精度：5%,1/8W","R143, R144, R153, R154",4,"pcs"]
[20,"贴片电阻","100K","0805R,精度：5%,1/8W","R145, R155",2,"pcs"]
[21,"插件可调电阻","10K精密可调电阻","RW1，3P，间距2.54","RW1",1,"pcs"]
[22,"贴片三极管","S8550","SOT23 ","Q4, Q5, Q6",3,"pcs"]
[23,"贴片二极管","1N4148","1206D","D2, D4, D60, D61",4,"pcs"]
[24,"贴片二极管","1N4007","1206D","D21, D22, D23",3,"pcs"]
[25,"贴片TVS管","SMBJ18.0CA","DO-214AA","D5, D6, D7, D8, D9, D10, D11, D12, D13, D14, D15, D16, D17, D18, D19, D20",16,"pcs"]
[26,"贴片TVS管","BV05C","SOD323","D52, D53, D54, D55, D56, D57, D58, D59",8,"pcs"]
[27,"贴片TVS管","SMBJ6.5CA","DO-214AA","D62, D63, D64, D65,D33",5,"pcs"]
[28,"贴片电感","10UH","1206","FB1, FB2, FB3",3,"pcs"]
[29,"贴片电感"," 600Ω/100MHz","0805","LH1, LH2, LH3, LH4, LH5, LH6, LH7, LH8, LH9, LH10, LH11, LH12, LH13, LH14, LH15, LH16, LH19, LH20, LH22,LH21, LH23",21,"pcs"]
[30,"贴片功率电感","30UH","L10*10","LH17, LH18",2,"pcs"]
[31,"贴片保险丝","SMD1812P200TF",1812,"F1, F4",2,"pcs"]
[32,"贴片保险丝","SMD1812P110TF","1812","F2, F5, F6, F7, F8, F9",6,"pcs"]
[33,"贴片发光二极管","LED","0805L","L1, L2, L3, L4, L5, L6, L7, L8, L9, L10, L11, L12, L13, L14, L15, L16, L17, L18, L19, L20, L33, L34, L35, L36, L37, L38,L21, L22, L23, L24, L25, L26, L27, L28, L29, L30, L31",37,"pcs"]
[34,"贴片反相器IC","74LVC04","SO-14","U19, U30",2,"pcs"]
[35,"贴片与门IC","SN74LVC08AD","SO-14","U1",1,"pcs"]
[36,"贴片485 IC","MAX3485E","SOP8","U28, U29",2,"pcs"]
[37,"插件485模块","RSM3485C-3.3V","RSM485C","U6, U7",2,"pcs"]
[38,"贴片232 IC","SP3223EEY","TSSOP-20","U8, U9, U10, U11",4,"pcs"]
[39,"贴片四光耦 IC","TLP521-4","TLP521-4","U12, U13",2,"pcs"]
[40,"贴片光耦 IC","HCPL-0600-500E","SOP8","U14, U15, U16, U17, U18",5,"pcs"]
[41,"贴片运放IC","OP491","SO-14","U20, U21",2,"pcs"]
[42,"贴片稳压IC","TL431ACLP","TO-92A","U23",1,"pcs"]
[43,"贴片AD采样 IC","TLC2543I","SOL-20","U24",1,"pcs"]
[44,"贴片3.3V IC","ASM1117M3-3.3","SOT223","U26",1,"pcs"]
[45,"贴片5.0V IC","ASM1117M3-5.0","SOT223","U27",1,"pcs"]
[46,"插件电源模块","WRB1205CS-3W","WRB_CS_3W","U25",1,"pcs"]
[47,"插件光耦","TL113","DIP6","O1, O2, O3",3,"pcs"]
[48,"插件继电器","G5LA-14 12V  DC","JZC-22F","K1, K2, K3",3,"pcs"]
[49,"插座RJ45*8","2*4,8口双层","RJ45-8C","J1, J2,J8",3,"pcs"]
[50,"插座8PIN","8PIN端子座","8SIP5.08","J4",1,"pcs"]
[51,"牛角连接器","HEADER 10X2","公头，2.54间距，直脚","J5",1,"pcs"]
[52,"牛角连接器","HEADER 13X2","公头，2.54间距，直脚","J7",1,"pcs"]
[53,"牛角连接器","HEADER 7X2","公头，2.54间距，直脚","J9",1,"pcs"]
[54,"牛角连接器","HEADER 10X2","母头，2.54间距，带扣",null,null,"pcs"]
[55,"牛角连接器","HEADER 13X2","母头，2.54间距，带扣",null,null,"pcs"]
[56,"牛角连接器","HEADER 7X2","母头，2.54间距，带扣",null,null,"pcs"]
[57,"RJ45+USB插座","RJ45+USB","RJ45-HRX-1","J10",1,"pcs"]
[58,"排针","3PIN-1","SIP3","JP3, JP4",2,"pcs"]
[59,"端子","XH2.54-2P","2.54间距，直脚","JP5",1,"pcs"]
[60,"端子","VH3.96-2p","直脚，带线长20cm ",null,null,"pcs"]
[61,"PCB板","A8_Inter_B ，大小：10.5*28cm\n","按PCB图下单，上传文件,材质：FR4，板厚：1.6cm，铜厚：1OZ",null,1,"pcs"]