[root@M28x NandFlash]# ./omAppSU SerManager new: 197528 AlmMngr init... AlmManager LoadChkItem: 127 AlmManager LoadAlmTime: 5 AlmManager LoadAlmRecv: 2 AlmManager LoadAlmDef: 13 AlmManager LoadAlmDev... AlmManager LoadAlmDev 联动1 GetSM type=2562 AlmManager LoadAlmDev GetSer OMI1: 0x800000 CSerDio::CSerDio: Dio Init AlmManager LoadAlmDev GetSer ok OMI1:[800001] open ok! AlmManager LoadAlmDev ser:OMI1: 800000 open:1 AlmManager LoadAlmDev 联动2 GetSM type=2562 AlmManager LoadAlmDev GetSer OMI1: 0x800000 CSerDio::CSerDio: Dio Init AlmManager LoadAlmDev GetSer ok OMI1:[800001] open ok! AlmManager LoadAlmDev ser:OMI1: 800000 open:1 AlmManager LoadAlmDev 联动3 GetSM type=2562 AlmManager LoadAlmDev GetSer OMI1 0x800000 CSerDio::CSerDio: Dio Init AlmManager LoadAlmDev GetSer ok OMI1[800001] open ok! AlmManager LoadAlmDev ser:OMI1 800000 open:1 AlmManager LoadAlmDev: 3 smtp: svr= acc= sub=机房报警 AlmMngr init end CSerDio::CSerDio: Dio Init CSerDio::CSerDio: Dio Init OMI1:[800001] open ok! OMI1:[800001] open ok! CSerCom InitCom: 1cf3c0 1 CSerCom UpdParams: ComPort: ttySP3, 0, 0 CSerCom UpdParams: ComPort: ttySP3, 0, 0 CSerCom::Open: /dev/ttySP3,9600,8,N,0 set serial done+! ttySP3:9600,n,8,1[100003] open ok! SEND: 7E 32 35 30 32 34 30 30 31 30 30 30 30 46 44 42 32 0D RECV: rcv=0 SEND: 7E 32 35 30 32 34 31 30 45 45 30 30 32 30 31 46 44 32 35 0D RECV: rcv=0 SEND: 7E 32 35 30 32 34 32 31 36 30 30 30 30 46 44 41 41 0D RECV: rcv=0 t=5121 iaddr=2 ver=25 brief=系统电压: V , 系统电流: A OMI1:[800001] open ok! OMI1:[800001] open ok! OMI1:[800001] open ok! OMI1:[800001] open ok! OMI1:[800001] open ok! OMI1:[800001] open ok! CSerCom UpdParams: ComPort: ttySP3, 0, 0 CSerCom::Open: /dev/ttySP3,9600,8,N,0 set serial done+! ttySP3:9600,n,8,1[100003] open ok! SEND: 7E 32 35 30 32 34 30 30 31 30 30 30 30 46 44 42 32 0D RECV: rcv=0 SEND: 7E 32 35 30 32 34 31 30 45 45 30 30 32 30 31 46 44 32 35 0D RECV: rcv=0 SEND: 7E 32 35 30 32 34 32 31 36 30 30 30 30 46 44 41 41 0D RECV: rcv=0 t=5121 iaddr=2 ver=25 brief=系统电压: V , 系统电流: A OMI1:[800001] open ok! OMI1:[800001] open ok! ^C [root@M28x NandFlash]#